**MDC-B Metal Detector**



**FEATURES**

1. Automatic adaptable for product effect.High attributes of products can be detected.
2. All-digital signal processing and transmission technology , high sensitivity, excellent reliability.
3. Based on 32bit high speed CPU.
4. Double LED line indicate the realtime Ferrous and Non-Ferrous sensitivity exactly.
5. Ferrous and Non-Ferrous level dividual adjustment.
6. Optional rejict systems.
7. High protection degree and height djustable frame.

**PURPOSE**

* Online metal detection for food product.A step for food safety(HACCP required)
* Also can fit for detecting the chemical products, rubber products.

**SPECIFICATIONS**

* Theory: Balanced Coil
* Adjustment: Auto and Ferrous and Non-Ferrous level dividual adjustment
* Aperture Size: 600\*80mm
* Alarm: Buzzer & Lamp
* Reject system: Air blast/air pusher/swing arm(option)
* Belt Speed:25-32m/min(Adjustment)
* Power:AC110V/220V 50-60HZ
* Rated Output: Appr140W
* Dimension:1620mm(L)\*1000mm(W)\*1100mm±50mm(H)
* Weight:Appr200Kg