**MDC-Symmetric**





**FEATURES**

* Based on High speed CPU control circuit, 320x240 resolution monochrome graphic LCD display, white text on a blue background
* Compact design with unique front cover and panel
* Adapt to touchpad integrated with key operation, Simple and durable
* Full-digital signal processing, high-precision measurement of signal
* Synchro Phase Angle adjustment
* Multi-stage signal stability circuit
* Automatic "self-teaching" function, compensating for product effect variations
* 20 kinds products memory, 1000 detection logs.
* Single-mode rejection time adjustment
* Adapt to worldwide voltages
* Protection grade IP65 (optional)

**SPECIFICATIONS**

* Theory: Balanced Coil
* Aperture Size:50mm×150mm
* Belt Speed:10-36m/min
* Reject System: Air blast/Arm Pusher/Swing Arm(option)
* Alarm: Buzzer&Lamp
* Power:AC110V/220V 50-60HZ
* Rated Output:120W
* Dimension：1850mm（L）×756mm（W）×985mm（H）±20mm
* Weight: Appr.140KG