**MDF Metal Detector**



**SPECIFICATION**

1. Model: MDF
2. Detection method: balanced coil.
3. Sensitive adjustment: automatic or manual.
4. Standard tube size: ￠120mm.
5. Alarm mode: buzzer and lamp (optional).
6. Reject method: Quick flap system.
7. Power: AC110V/220V 50-60HZ.
8. Power: 200W.
9. Dimensions: 420mm(L)\*500mm(W)\*1300±10mm(H).
10. Weight: Appr. 88kg

**FEATURES**

1. Stainless Steel Conveyor with high waterproof level design.
2. 100 Product Preset; Easy to shift or edit.
3. 2000 logs memory, easy to look up and print out.
4. Based on friendly touch screen operation.
5. High speed metal detection unit.
6. Multi-function operation system and multi-language for option.
7. Advanced product’s effective learn.
8. Variety of peripheral system connection and setup.
9. Detection frequency optional.(Factory preset).
10. Special reject system design, suitable for powder and granular bulk materials.