**MDP Metal Detector**



**Product specifications**

* Model: MDP
* Theory: Balance Coil.
* Sensor adjustment:Self-study and manual adjustment.
* The standard diameter: 100 \* 40 (mm).
* Alarm:Buzzer & Lamp (optional).
* Reject system:Rapid isolation shield.
* Power:AC110V/220V 50-60HZ.
* Rated Output: Appr 200W.
* Dimension:700mm (L) \* 760mm (W) \* 1200 ± 10mm (H).
* Weight:Appr 88Kg.

**FEATURES**

* Suitable for high speed drug particles testing.
* Consistent with the pharmaceutical industry hygiene requirements with high-performance tablet 3,Tablet press, capsule filling machine combines.
* Man-Machine Interface, User-friendly operation
* Can be set to 100 species.
* Automatically or manually adjust the sensitivity.
* Automatic learning function, compensation of the "product effect"
* 1000 records.
* Record data printing.
* A special rejection device designed for powdery and granular bulk materials.
* Excluding metal impurities, ensuring the production line working well.
* Adjustable for height and angle to facilitate the production line installation.
* high-speed cylinder control, fast response.